Type: ISOR 500 E4 20

Item number: 132574

Description:

Fully insulated fan box for mounting in ventilation tubes. For easy mounting in tubes, the connecting pieces are provided with a lip seal. Housing made of galvanized sheet steel with sound-absorbing inner lining of 40 mm mineral wool with abrasion resistant glass fiber coating according to DIN EN 13 501-1 Class A1. Mounting position horizontally and vertically possible. Through a removable cap, the swing-out fan unit is easy to clean. Ventilator unit easily removable from the

sound proof casing. With integrated mounting bracket for easy installation.

An efficiency-optimized impeller with backward curved blades is fitted on the external rotor of a voltage controllable motor. The impeller is balanced according to the quality class G 6.3 of DIN / ISO 1940, on 2 planes. Closed drive motor, maintenance-free ball bearings with lifetime lubrication, sealed on both sides. All fans with standard motor protection using thermal contact and internally connected motor capacitor. The electrical connection is to be done via an external terminal box.

CE marking according to EC Declaration of Conformity for Electromagnetic Compatibility EMC - Directive 2004/108/EC. EC - Declaration of Incorporation according to the Machinery Directive 2006/42/EC - Directive 2009/125/EC (Reg.

1253/2014/EU).

Technical data:

Volumetric flow (V): m³/h Pressure increase (Δp fa): Pa Efficiency static max. (η fa): 40,6 % Efficiency total max. (ηt): 41,2 %

Rated voltage (U): 230, 1~ V Rated frequency (f): 50 Hz Rated power consumption (P N): 466 W Current consumption max. (I max.): 2,7 A

Rated speed (n): 1350 min-1

Protection class motor: IP 54

Protection class terminal box: IP 44

Ambient temperature max. (t A): 65 °C Medium temperature max. (tM): 65 °C

Casing sound power level (L WA2): 58 dB(A) Inlet sound power level (L WA5): 67 dB(A) Outlet sound power level (LWA6): 72 dB(A)

Dimensions (L x W x H): 800x783x587 mm Connection diameter: 500 mm Weight: 69,5 kg

Wiring diagram: 116495

Manufacturer:

ruck Ventilatoren GmbH Max-Planck-Str. 5

97944 Boxberg

Tel. 07930-9211300 [www.ruck.eu](http://www.ruck.eu/)

Type: ISOR 500 E4 20

Item number: 132574

|  |  |  |
| --- | --- | --- |
| Available accessories:VM 500 | 118094 | Fast clamps, 1 set = 2 pcs., size 500 |
| SDS 500 | 118834 | Silencer rigid, 1m, sound insulation 50mm, size 500 |
| SG 500 01 | 134286 | Protection grille size 500 |
| RD ISOR 03 | 130517 | Rain cover for ISOR |
| GS 01 | 102787 | Isolator switch |
| TEM 035 | 103502 | 5-step transformer box with connection for motor protection, IP54 |
| TES 035 | 103954 | 7-step transformer without motor protection, for switch cabinet, IP20 |